1

1

Audio/V ideo Transport

Working Group

41st IETF, Washington, DC

1 April 1998

S tephen Casner

Precept Software

Wednesday Agenda

l Des ign fudge factor to converge to desired value in timer recons ideration l Ignore premature timeouts on s tep leave l Add fac tor to correct for low estimate w ith sampled

SSRC algorithm when size decreases l Define SDP BW modifiers to specify ex plicit RTC P s ender and receiver B W l Add RTCP minimum interval sc aling as a ^MAY~ l Specify ^ relative~ NTP uses ^best~ platform clock l Specify P -bit padding for RTC P only on last packet

Issues from Mailing L ist l Additional SDES items

» PHOTO URL, home page URL

» Nick-name

» Organization l Request for RTCP RR extensions l Rev ising definition of RR ^loss fraction~

RTCP RR Packet

0 31

prof ile-specific fixed portion

P RC RR length(32-bit wds)

fixed portion

RC- long array of blocks

prof ile-specific array of blocks

RTCP RR App. Extensions

l Request to add application-specific

sec tion following profile-specific section

l Identify app by 32-bit FOURCC in first

word, registered with IANA

l Presume only one application-specific

extension allowed in any RR

l Alternative is to put same info in APP

packet -- adds 8 by tes

RTCP RR ^loss fraction~

l Cur rently defined to be ov er the whole

RTCP interval sinc e last report

l Change definition to a shorter interval:

» scaled with BW for constant number of bits

» constant time (2minutes? 30 seconds?)

» exponential avg withhalf-life of 128 pkts

» filterspecified in SDP

l Can we get it ^right~?

Advancing Profile t o Draft Std

l From Memphis: specify SHOULD use

numeric format for CNAME - still agree?

l Allow default 5% RTCP bandwidth to be

overridden

l New draft has more complete encoding

list and descriptions

l May need changes for generic formats