Nächste Seite: Georeferenzierung einer unverzerrten nicht Aufwärts: Lösung mit GRASS Vorherige Seite: PNG-Format Inhalt Index

## Georeferenzierung einer unverzerrten ausgerichteten Rasterdatei

Im diesem Fall reicht es zur Georeferenzierung aus, die Nord-, Süd-, West- und Ostwerte der Bildkanten an GRASS zu übergeben. Dies geschieht mit dem Befehl `r.support`, da die importierten Bilddateien als Raster gespeichert sind. Nach dem Aufruf an der Kommandozeile fragt der Befehl nach der zu bearbeitenden Rasterdatei. Durch Eingabe von `list` können vorhandene Dateien angezeigt werden. Hat man die gewünschte Datei ausgewählt, fragt das Programm, ob der Header der Datei bearbeitet werden soll; dieses bejaht man. Die Aufforderung `hit RETURN to continue` ignoriert man und drückt die `ESC-Taste` gefolgt von einem `ENTER` um die Auflösungsparameter bearbeiten zu können. Nun bekommt man Informationen über die Auflösung der Rasterdatei rows = Reihen oder Spalten , cols = Zeilen und die Farbtiefe in Byte bytes per cell. Durch Eingabe von `ESC` und `ENTER` kommt man zu der eigentlichen Georeferenzierung. Der CELL HEADER ist Träger der Geoinformation einer Rasterdatei in GRASS. Zur Orientierung wird die Ausdehnung der Region bzw. des Mapset ausgegeben. Die Bestätigung der Eintragungen erfolgt durch `ESC` gefolgt von `ENTER`. Die weiteren Abfragen können mit `ENTER` bestätigt werden.
HeaderDer Header (Kopf) eines Dateiformates enthält grundsätzliche Angaben über die in dem Dateiformat gespeicherten Daten.

    GRASS:/spare/gisdata/grass/bin > r.support

    Enter name of raster file for which you will create/modify support files
    Enter 'list' for a list of existing raster files
    Enter 'list -f' for a list with titles
    Hit RETURN to cancel request
    > craterluft
    <craterluft>
    Edit the header for [craterluft]? (y/n) [y]
    Edit header for [craterluft]
    cellhd compression: 1
    3.0 compression indicated
    pre 3.0 compression not indicated

    hit RETURN to continue -->

    Please enter the following information for [craterluft]

     4207   Number of rows
     4123_  Number of cols
     2____  Number of bytes per cell

               AFTER COMPLETING ALL ANSWERS, HIT <ESC><ENTER> TO CONTINUE
                                (OR <Ctrl-C> TO CANCEL)

Importiert man die Rasterdaten mit dem schon in Kapitel 4 vorgestellten Befehl `r.in.gdal` so wird gleich eine passende Default Region erzeugt. So würden auch die Warnungen warning - north falls outside the default region und warning - east falls outside the default region wegfallen.

                               IDENTIFY CELL HEADER

               ============================= DEFAULT REGION ========
               |          Default North:1                          |
               |                                                   |
               |           =======  CELL HEADER  =======           |
               |           | NORTH EDGE:4775100____    |           |
               |           |                           |           |
     Def. West |WEST EDGE  |                           |EAST EDGE  | Def. East
     0         |550840_____|                           |592070_____| 1
               |           | SOUTH EDGE:4733020____    |           |
               |           =============================           |
               |                                                   |
               |          Default South:0                          |
               =====================================================
               PROJECTION: 1 (UTM)                        ZONE: 10

               AFTER COMPLETING ALL ANSWERS, HIT <ESC><ENTER> TO CONTINUE
                                (OR <Ctrl-C> TO CANCEL)

      projection:   1 (UTM)
      zone:         10
      north:       4775100
      south:       4733020
      east:        592070
      west:        550840

      e-w res:     10
      n-s res:     10

      total rows:             4200
      total cols:             4100
      total cells:      17,000,000

    warning - north falls outside the default region
    warning - east falls outside the default region

    Do you accept this header? (y/n) [n] >y
    header for [craterluft] updated

    hit RETURN to continue -->
    Update the stats (histogram,range) for [craterluft]? (y/n) [n] y

    Edit the category file for [craterluft]? (y/n) [n] n
    Create/Update the color table for [craterluft]? (y/n) [n] n
    Edit the history file for [craterluft]? (y/n) [n] n
    The null file for [craterluft] might indicate that some cells contain
    no data. If null file for [craterluft] doesn't exist all
    zero cells in [craterluft]
    are treated by GRASS application programs as no data.

    Do you want to create/reset null file for [craterluft] so that
    all cell values are considered valid data? (y/n) [n] n

    Do you want to delete null file for [craterluft]
    (all zero cells will then be considered no data)? (y/n) [n] n

Nächste Seite: Georeferenzierung einer unverzerrten nicht Aufwärts: Lösung mit GRASS Vorherige Seite: PNG-Format Inhalt Index