ISO/IEC JTC 1/SC6 N 7532

Disposition of Comments on Defect Report

ISO/IEC 9542/014

1 Introduction

The Defect Report ballot for ISO/IEC 9542/014 (SC6 N6824) closed on 1992-04-17. The summary of voting is

contained in document SC6 N7265. There were 9 approval votes (Brazil, Canada, Denmark, Finland, Germany,

Japan, Sweden, USA), no approval with comments, 2 disapprovals (France, UK), 1 abstention (Italy), and 7 bal-

lots not returned (Australia, Belgium, Korea, Netherlands, Romania, Russian Federation).

Ballot results and member body comments were discussed and resolved successfully at the San Diego meeting of

SC6/WG2. Experts from the member bodies submitting comments were present for the discussions. All com-

ments were successfully resolved and replacement text agreed for a Technical Corrigendum to the standard.

2 Resolution of specific member body comments

2.1 France Comments

Comment 1: The French comment expressed concern that the proposed defect resolution constituted an en-

hancement to the protocol and not simply a defect correction. It was agreed by the editing

group that indeed the French concern was justified, but that by adopting the approach proposed

by the UK in their comment 1, this concern would be eliminated. Since the editing group con-

curred with the essence of the UK replacement text, the comment from France was accommo-

dated.

2.2 UK Comments

Comment 1: This comment was the basis for the UK negative vote on the defect report. The rationale be-

hind the UK position was accepted by the editing group as the basis for rejecting the proposed

defect resolution in the balloted defect report. The UK proposed alternate replacement text

which was accepted, with modification, as the basis for a Technical Corrigendum to the stan-

dard. Thus, this UK comment was accommodated.

Comment 2: The UK also expressed concern that, even with the proposed replacement text to correct the

problem with allowing enhancement to ISO/IEC 9542 by adding new PDU types, that the stan-

dard would still not be sufficiently �future proof�. After discussion the editing group devel-

oped a simple approach to better support future extension of the protocol while preserving

complete backwards compatibility with implementations conforming to the published stan-

dard. The proposal divides the PDU type code space for ISO/IEC 9542 into two ranges. The

range containing all the existing PDU types would have the behavior specified in the UK pro-

posed replacement text; the other range could be used for future extension of the protocol to

ISO/IEC JTC 1/SC6 N 7532

incorporate PDU types which would generate a protocol error if received by an implementation not

supporting the extended protocol.

Comment 3: This comment reflected on the consequences of having made ISO/IEC 9542 a separate protocol

type from ISO/IEC 8473, while incorporating a similarly �distinct� protocol for address admini-

stration as part of the ISO/IEC 9542 protocol. It cautioned that in the future it would be desirable to

give more thought to whether extended functions should be incorporated into an existing protocol

specification and sharing the protocol type of that protocol, or be considered a separate protocol

with its won protocol type. Since this comment was philosophical in nature and did not affect the

approach taken to resolving the subject defect, the point was noted to be considered in the develop-

ment of future OSI protocols.

3 Replacement text for ISO/IEC 9542

Add the following text at the end of clause 7.2.5:

�If a PDU is received with a reserved PDU type value in the range 10000 to 11111, it

shall be treated as invalid and therefore as constituting a protocol error. If a PDU is re-

ceived with a reserved PDU type in range 00000 to 01111, then it may either:

a) be considered as valid but entirely ignored, or

b) be treated as invalid, and therefore constituting a protocol error.

NOTE - It is recommended that PDUs having type values in the range 00000 to 01111

should be ignored rather than treated as invalid, because this would be the most appropri-

ate behaviour in view of the envisaged use of these type values in protocol enhance-

ments.�