Nächste Seite: Das Modul v.digit Aufwärts: Maskierung des befahrenen Hafengebietes Vorherige Seite: Maskierung des befahrenen Hafengebietes Inhalt Index

#### Alternativer Lösungsweg

Als Alternative zu der folgenden ,,manuellen`` Labelung der Fläche wurde von Andreas Lange ein weiterer Lösungsweg aufgezeigt, der in wenigen Kommandos den manuellen Arbeitsablauf automatisiert. Die optionale Nutzung von v.digit wird als Beispiel für die möglichen Lösungen im Tutorial belassen. Der Befehl `v.alabel` bewirkt eine Massenbenennung aller vorhandenen areas in der aufgerufenen Vektordatei. Mit einem optional anzuhängenden `value=`gewünschter Wert kann die per Grundeinstellung vergebene 1 geändert werden. Das Kommando `v.support` wird automatisch ausgeführt. Nun kann der anschließende Abschnitt Das Modul v.digit übersprungen und direkt mit der Umwandlung von Vektor- in Rasterdaten (Seite ) fortgefahren werden.

    GRASS:/spare/gisdata/grass/bin > v.alabel map=test
    Labeled 1 new areas.

    Running support now...

    V.SUPPORT:

    Selected information from vector header
     Organization:
     Map Name:      Convex hull map
     Source Date:
     Orig. Scale:   2400
     No snapping will be done

        Reading Vector file 100%
        Building areas 100%
        Building islands 100%
        Attaching labels
     Number of lines:   1
     Number of nodes:   1
     Number of areas:   1
     Number of isles:   1
     Number of atts :   1
     Number of unattached atts :   0
     Snapped lines  :   0

Hier endet der alternative Lösungsweg zur Labelung von areas.