Nächste Seite: Anzeigen der Höhenlinien Aufwärts: Lösung mit GRASS Vorherige Seite: Lösung mit GRASS Inhalt Index

## Erzeugen der Höhenlinien

Zum Erzeugen von Höhenlinien verwendet man den Befehl r.contur. Hiermit werden Konturlinien aus einer Rasterdatei erzeugt. Diese Konturlinien werden in einer Datei im GRASS-Vektorformat output= gespeichert. Mit step= wird die Äquidistanz, also das Intervall zwischen den Konturlinien vorgegeben.
Es können aber auch direkt die auszugebenden Konturlinien benannt werden levels= , , , . Die Auswahl eines Bereiches für den die Höhenlinien erzeugt werden sollen, ist durch die Definition einer Untergrenze minlevel= und einer Obergrenze maxlevel= möglich.

    GRASS: > r.contour -n input=crater output=hlinien step=150
    Reading data.
    Percent complete:  100%
    FPRange of data:    min =  0.000000 max = 2721.000000
    Minimum level will be 0.000000
    Maximum level will be 2700.000000
    Continue?(y/n) [y] y
    Displacing data.
    Percent complete:  100%
    Total levels:   19   Current level:

    Building topology...

       V.SUPPORT:

    Selected information from vector header
     Organization:
     Map Name:      from raster map crater
     Source Date:
     Orig. Scale:   0
     No snapping will be done

        Reading Vector file.
     100%
        Building areas
        Building islands
        Attaching labels
     Number of lines:   261
     Number of nodes:   262
     Number of areas:   0
     Number of isles:   0
     Number of atts :   261
     Number of unattached atts :   0
     Snapped lines  :   0

    Finished.