Nächste Seite: Tipps: Aufwärts: Punktdaten durch Interpolation in Vorherige Seite: Mit s.surf.rst Inhalt Index

#### Tipps

- Mit den Optionen der Interpolationsbefehle sollte nicht sorglos umgegangen werden. Es wird hier auf die Aufsätze[6] der beteiligten Entwicklerin Helena Mitasova sei hier verwiesen.

Abbildung 3.3: GRASS-Monitor mit den interpolierten Rastertiefendaten ,,Hafen Elsfleth`` aus dem Modul `s.surf.idw`
.

    GRASS:~ > s.surf.rst input=tiefen elev=grund maskmap=MASK /
    tension=100 segmax=700

    Authors: original version L.Mitas, H.Mitasova
             GRASS implementation I.Kosinovsky, D.P.Gerdes
    see references in manual page or at:
    http://www2.gis.uiuc.edu:2280/modviz/papers/listsj.html

    Warning: strip exists with insufficient data

    The number of points in sites file is 493
    The number of points outside of region 0
    The number of points being used (after reduction) is 493

    Processing all selected output files
    will require 4294168 bytes of disk space for temp files

    bitmap mask created
     100%
    Percent complete: history initiated
    GRASS:~ >

Ist der an der Kommandozeile übergebene Parameter `tension=` zu klein gewählt, die Defaulteinstellung ist hier `tension=40`, kann es bei starken Änderungen der Höhenwerte zu einer Overshoot - Warnung des Programmes kommen. Siehe folgendem Beispielaufruf. Diese besagt das es mit den eingestellten Werten nicht möglich ist eine geglättete Oberfläche zu erzeugen. Durch die Erhöhung des entsprechenden Parameters kann dieser Warnung abgeholfen werden. Auch hier sollten den schon erwähnten Literaturhinweisen und Manual-Pages beachtung geschenkt werden.

    GRASS:~ > s.surf.rst input=tiefen elev=grund maskmap=MASK segmax=700

    Authors: original version L.Mitas, H.Mitasova
             GRASS implementation I.Kosinovsky, D.P.Gerdes
    see references in manual page or at:
    http://www2.gis.uiuc.edu:2280/modviz/papers/listsj.html

    Warning: strip exists with insufficient data

    The number of points in sites file is 493
    The number of points outside of region 0
    The number of points being used (after reduction) is 493

    Processing all selected output files
    will require 4294168 bytes of disk space for temp files

    bitmap mask created
    WARNING:
    Overshoot -- increase in tension suggested.
    Overshoot occures at (483,664) cell
    The z-value is -1.972525,zmin is -8.160000,zmax is -2.600000
     100%
    Percent complete: history initiated